**Product** **Specifications**

**RW SERIES**

**P3.9 Budget Rental display**

**![A picture containing indoor, table, sitting, monitor

Description automatically generated]()**

**Overview**

Vanguard’s RW Series is the perfect combination of price point and resolution for today’s competitive DVLED market. When lead time and price point are the most important factors, Vanguard’s RW series cannot be beat. Available in a P3.9 rental style cabinet, RW is the perfect cabinet to create unique elements on a stage while providing the ability to reconfigure as often as desired.

**Additional Features**

* Rear Service Only.
* Flyable or ground-stackable.
* Easy installation.
* Light but durable cabinet.
* Extremely cost competitive.
* Lead times as short as 2 weeks.

**Specifications**

RW Indoor P3.9

ENVIRONMENTAL

Operating Temperature -10°C to +50°C

Storage Temperature -20°C to +60°C

Operating Humidity 20% to 90% RH

LED

Pixel Density 65,536/m²

LED Type SMD1R1G1B

Modules Per Cabinet 4

Lifetime to Half Brightness (L50) 100,000

Contrast Ratio 2,000:1

Brightness 800 Nits

Viewing Angle 140° x 140°

CABINET

Cabinet Material Aluminum

Cabinet Size 19.69” x 19.69” x 3.3”

Cabinet Resolution 128 x 128

Modules Per Cabinet 1

Cabinet Weight 19.2 lbs.

Service Access Rear Only

IP Rating IP30

cccc

INTERNAL OPERATION

Gray Scale 14bit

Refresh Rate >3840Hz

Frame Frequency 60Hz

AC POWER

Source Voltage 100-240V, 50/60Hz

Max Power Consumption 200W

Avg. Power Consumption 100W